Cracking Projects For Newbies

FAKE SERIAL in registry Sunday, 07-Feb-99 18:01:28 195.36.143.98 writes: When we change the [esp+10] to [esp+14] we only change what is in the memory when the COMPARISON is done, but we don't change the value of the memory content, so when it writes the serial to registry, we still have our fake serial in [esp+10]. I hope it helps :) Friendly HarvestR

Message thread:

Jeff: jas's Thread for NEW newbys (05-Feb-99 21:20:24)

Cigam: Why the copy is unreged after running original (05-Feb-99 21:53:49)
Jeff (jas): Re: jas's Thread for NEW newbys; Changing registers in ICE; (06-Feb-99 15:18:05)

HarvestR: Re: Changing registers in ICE; nice jeff :) (06-Feb-99 18:48:06)

Jeff: Re: Re: Changing registers in ICE; MayBE NOT! (07-Feb-99 02:13:18)

Princess: Re: Re: Re: Changing registers in ICE; MayBE NOT! (07-Feb-99 09:19:29)

Jeff: Re: Re: Re: Re: Changing registers in ICE; MayBE NOT! (07-Feb-99 11:58:09)

Jeff: Re:Changing registers in ICE; NEW Question (07-Feb-99 12:18:42)

Jeff(jas): Re: Task# 3; written for new Newbys; boring for 'oldies' :) (07-Feb-99 17:20:12)

Jeff: Re: Re: Task# 3; CORRECTIONS (08-Feb-99 12:31:06)

Princess: Re: Re:Changing registers in ICE; NEW Question (07-Feb-99 17:35:18)
HarvestR: FAKE SERIAL in registry (07-Feb-99 18:01:28)

Jeff: Re: FAKE SERIAL in registry (08-Feb-99 15:14:33)

Jeff: Re: BTW; My best Game so far; (08-Feb-99 16:04:00)

Back to main board

Message subject: Name: (optional) Email address: (optional) Type your message here:

Back to main board

Copyright © InsideTheWeb, Inc. 1997-1999
All rights reserved.