Cracking Projects For Newbies

Re: Re: Re: Changing registers in ICE; MayBE NOT! Sunday, 07-Feb-99 09:19:29 206.248.47.45 writes: Hi Jeff Yes it works as you described. If you change the 10 to 14 by editing in softice. As long as you have the program open it will work fine,however when you exit the program it will revert to its original state. Did you make the patch permanent in your hex editor ?? Princess Princess

Message thread:

Jeff: jas's Thread for NEW newbys (05-Feb-99 21:20:24)

Cigam: Why the copy is unreged after running original (05-Feb-99 21:53:49)
Jeff (jas): Re: jas's Thread for NEW newbys; Changing registers in ICE; (06-Feb-99 15:18:05)

HarvestR: Re: Changing registers in ICE; nice jeff :) (06-Feb-99 18:48:06)

Jeff: Re: Re: Changing registers in ICE; MayBE NOT! (07-Feb-99 02:13:18)

Princess: Re: Re: Re: Changing registers in ICE; MayBE NOT! (07-Feb-99 09:19:29)

Jeff: Re: Re: Re: Re: Changing registers in ICE; MayBE NOT! (07-Feb-99 11:58:09)

Jeff: Re:Changing registers in ICE; NEW Question (07-Feb-99 12:18:42)

Jeff(jas): Re: Task# 3; written for new Newbys; boring for 'oldies' :) (07-Feb-99 17:20:12)

Jeff: Re: Re: Task# 3; CORRECTIONS (08-Feb-99 12:31:06)

Princess: Re: Re:Changing registers in ICE; NEW Question (07-Feb-99 17:35:18)
HarvestR: FAKE SERIAL in registry (07-Feb-99 18:01:28)

Jeff: Re: FAKE SERIAL in registry (08-Feb-99 15:14:33)

Jeff: Re: BTW; My best Game so far; (08-Feb-99 16:04:00)

Back to main board

Message subject: Name: (optional) Email address: (optional) Type your message here:

Back to main board

Copyright © InsideTheWeb, Inc. 1997-1999
All rights reserved.